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ITEM 7.01 REGULATION FD DISCLOSURE

On June 30, 2014 General Motors Company (GM) issued a press release regarding safety recalls of approximately 7.6 million vehicles in the U.S. covering certain models from the 1997 to 2014 model years. GM expects to take a charge of up to approximately $1.2 billion in the three months ended June 30, 2014 for the cost of recall-related repairs announced in the quarter. This amount includes a previously disclosed $700 million charge for recalls announced May 15, 2014, May 20, 2014 and June 16, 2014. The GM press release is incorporated as Exhibit 99.1.

ITEM 9.01 FINANCIAL STATEMENTS AND EXHIBITS
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	Press Release
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For Immediate Release: Monday, June 30, 2014


GM Announces Six Safety Recalls

DETROIT - General Motors announced today it will conduct six new safety recalls in the United States involving about 7.6 million vehicles from the 1997 to 2014 model years.

“We undertook what I believe is the most comprehensive safety review in the history of our company because nothing is more important than the safety of our customers,” said GM CEO Mary Barra. “Our customers deserve more than we delivered in these vehicles. That has hardened my resolve to set a new industry standard for vehicle safety, quality and excellence.”

Among these recalled vehicles, GM is aware of seven crashes, eight injuries and three fatalities. The fatal crashes occurred in older model full-size sedans being recalled for inadvertent ignition key rotation. There is no conclusive evidence that the defect condition caused those crashes.

“We have worked aggressively to identify and address the major outstanding issues that could impact the safety of our customers,” Barra said. “If any other issues come to our attention, we will act appropriately and without hesitation.”

GM has made changes to every process that affects the safety of its vehicles, and the company has acted or will act on all 90 of the recommendations put forward by former U.S. Attorney Anton Valukas in his independent report to the company’s Board of Directors.

GM expects to take a charge of up to approximately $1.2 billion in the second quarter for the cost of recall-related repairs announced in the quarter. This amount includes a previously disclosed $700 million charge for recalls already announced during the quarter.

Until the ignition recall repairs have been performed, it is very important that customers remove all items from their key ring, leaving only the vehicle key, and always use their seat belts. The key fob, if present, should also be removed from the key ring.


General Motors Co. (NYSE:GM, TSX: GMM) and its partners produce vehicles in 30 countries, and the company has leadership positions in the world's largest and fastest-growing automotive markets. GM, its subsidiaries and joint venture entities sell vehicles under the Chevrolet, Cadillac, Baojun, Buick, GMC, Holden, Jiefang, Opel, Vauxhall and Wuling brands. More information on the company and its subsidiaries, including OnStar, a global leader in vehicle safety, security and information services, can be found at http://www.gm.com


Forward-Looking Statements

In this press release and in related comments by our management, our use of the words “expect,” “anticipate,” “possible,” “potential,” “target,” “believe,” “commit,” “intend,” “continue,” “may,” “would,” “could,” “should,” “project,” “projected,” “positioned” or similar expressions is intended to identify forward-looking statements that represent our current judgment about possible future events. We believe these judgments are reasonable, but these statements are not guarantees of any events or financial results, and our actual results may differ materially due to a variety of important factors. Among other items, such factors might include: our ability to realize production efficiencies

and to achieve reductions in costs as a result of our restructuring initiatives and labor modifications; our ability to maintain quality control over our vehicles and avoid material vehicle recalls; our ability to maintain adequate liquidity and financing sources and an appropriate level of debt, including as required to fund our planned significant investment in new technology; the ability of our suppliers to timely deliver parts, components and systems; our ability to realize successful vehicle applications of new technology; and our ability to continue to attract new customers, particularly for our new products. GM's most recent annual report on Form 10-K and quarterly reports on Form 10-Q provides information about these and other factors, which we may revise or supplement in future reports to the SEC.

###

CONTACTS:

Alan Adler

GM Communications

313-319-8486

alan.adler@gm.com

Jim Cain

GM Communications

313-407-2843

james.cain@gm.com

GM ANNOUNCES SIX RECALLS, JUNE 30, 2014

	
	
	
	U.S.
	GMNA

	#
	MY/MODELS
	CONDITION
	POPULATION
	POPULATION

	1
	1997-2005 Chevrolet Malibu;
	Unintended ignition key rotation
	6,805,679
	7,610,862

	
	1998-2002 Oldsmobile Intrique;
	
	
	

	
	1999-2004 Oldsmobile Alero;
	
	
	

	
	1999-2005 Pontiac Grand Am;
	
	
	

	
	2000-05 Chevrolet Impala and Monte Carlo;
	
	
	

	
	2004-08 Pontiac Grand Prix
	
	
	

	
	
	
	
	

	2
	2003-14 Cadillac CTS, 2004-06 Cadillac SRX
	Unintended ignition key rotation
	554,328
	616,179

	3
	2011-14 Chevrolet Cruze; 2012-14 Chevrolet Sonic;
	On certain vehicles, insulation on the engine block
	2,990
	20,134

	
	2013-14 Chevrolet Trax, Buick Encore and Verano
	heater power cord (if equipped) may become damaged
	
	

	
	
	during very cold conditions.
	
	

	
	
	
	
	

	4
	2014 Chevrolet Camaro and Impala, Buick Regal,
	Some vehicles may not have had a “Superhold” joint
	106
	117

	
	Cadillac XTS
	fastener torqued to specification at the assembly plant.
	
	

	5
	2007-11 Chevrolet Silverado HD, GMC Sierra HD
	An overload in the feed may cause the underhood
	9,371
	12,008

	
	equipped with an auxiliary battery
	fusible link to melt due to electrical overload, resulting
	
	

	
	
	in potential smoke or flames that could damage the
	
	

	
	
	electrical center cover and/or the nearby wiring harness
	
	

	
	
	conduit.
	
	

	
	
	
	
	

	6
	2005-07 Buick Rainier, Chevrolet TrailBlazer, GMC
	A possible electrical short in the driver’s door module
	181,984
	188,705

	
	Envoy, Isuzu Ascender, Saab 9-7x;
	that could disable the power door lock and window
	
	

	
	2006 Chevrolet TrailBlazer EXT, GMC Envoy XL
	switches and, in rare cases, overheat the module.
	
	

	
	
	
	U.S.TOTAL
	GMNA

	
	
	
	
	TOTAL

	
	
	
	
	

	
	
	
	7,554,458
	8,448,005
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